The test cases here are described using Gherkin syntax, a non-technical, human readable language

The tests are ordered by opcode

# 0x42: Test\_SNN

|  |  |
| --- | --- |
| Given: | The unit under test is in setup mode, and the valid node number |
| When: | The cbus message SNN is sent |
| Then: | Expect to receive a NNACK message from the unit under test |
| Additional: |  |

# 0x4F: Test\_NNRSM

|  |  |
| --- | --- |
| Given: | The node number of the unit under test |
| When: | The cbus message NNRSM is sent |
| Then: | Expect to receive a GRSP OK message from the unit under test, with the same node number |
| Additional: |  |