The test cases here are described using Gherkin syntax, a non-technical, human readable language

The tests are ordered by opcode

# 0x0D: Test\_QNN

|  |  |
| --- | --- |
| Given: | The node number of the unit under test |
| When: | The cbus message QNN is sent |
| Then: | Expect to receive a PNN message from the unit under test |
| Additional: | If successful, store the content of the PNN for use by subsequent tests |